 GS 3060R2L Array (192.168.1.72)
	System Information
		Controller Time: 09/05/2023 10:25 AM
		Configuration password: Yes
		Maintenance password: Yes
		Total Cache Size: 128GB (ECC DDR)
		Firmware Version: 1.49C.14
		BIOS Version 1.11H
		Event Version: 20201127
		Controller Position: Slot A
		Service ID: 9146147
		Slot A Serial Number: 9148029
		Slot B Serial Number: 9148028
		Cache Backup Module: Cache Backup Module charging OFF (battery fully charged)
		Cache Backup Module (Redundant): Cache Backup Module charging OFF (battery fully charged)
		ID of NVRAM Defaults: V2.85.300
		Host Board - Slot A: FC 16G (SN: 9147244 (0x8B936C))
		Host Board - Slot B: FC 16G (SN: 9147235 (0x8B9363))
		I2C Device
			Device Name: PSU0
			Value:
			Status: PSU0 functioning normally
		I2C Device
			Device Name: PSU1
			Value:
			Status: PSU1 functioning normally
		I2C Device
			Device Name: Cooling Fan0
			Value:
			Status: Cooling Fan0 is in lowest speed
		I2C Device
			Device Name: Cooling Fan1
			Value:
			Status: Cooling Fan1 is in lowest speed
		I2C Device
			Device Name: Cooling Fan2
			Value:
			Status: Cooling Fan2 is in lowest speed
		I2C Device
			Device Name: Cooling Fan3
			Value:
			Status: Cooling Fan3 is in lowest speed
		I2C Device
			Device Name: Backplane Temperature
			Value: 49.0 C
			Status: Temp. within safe range
		Controller Device (Redundant)
			Device Name: CPU Temperature (Redundant)
			Value: 59.0 C
			Status: Temp. within safe range
		Controller Device (Redundant)
			Device Name: Controller Temperature(1) (Redundant)
			Value: 53.0 C
			Status: Temp. within safe range
		Controller Device (Redundant)
			Device Name: Controller Temperature(2) (Redundant)
			Value: 62.0 C
			Status: Temp. within safe range
		Controller Device (Redundant)
			Device Name: Controller Temperature(3) (Redundant)
			Value: 62.5 C
			Status: Temp. within safe range
		Controller Device (Redundant)
			Device Name: +5V Value (Redundant)
			Value: 5.062 V
			Status: Voltage within acceptable range
		Controller Device (Redundant)
			Device Name: +12V Value (Redundant)
			Value: 12.175 V
			Status: Voltage within acceptable range
		Controller Device (Redundant)
			Device Name: FC 16G (Redundant)
			Value:
			Status: FC 16G functioning normally
		Controller Device
			Device Name: CPU Temperature
			Value: 62.5 C
			Status: Temp. within safe range
		Controller Device
			Device Name: Controller Temperature(1)
			Value: 55.0 C
			Status: Temp. within safe range
		Controller Device
			Device Name: Controller Temperature(2)
			Value: 56.0 C
			Status: Temp. within safe range
		Controller Device
			Device Name: Controller Temperature(3)
			Value: 67.0 C
			Status: Temp. within safe range
		Controller Device
			Device Name: +5V Value
			Value: 5.016 V
			Status: Voltage within acceptable range
		Controller Device
			Device Name: +12V Value
			Value: 12.013 V
			Status: Voltage within acceptable range
		Controller Device
			Device Name: FC 16G
			Value:
			Status: FC 16G functioning normally
	Controller Setting(s)
		Controller Name: Not Set
		Logo: GS 3060
		Model: GS 3060R2L
		Vendor: Infortrend
		Raid Unique Identifier: 757539(0xB8F23)
		Time Zone: -08:00
		Date/Time: 2023-09-05 10:25
		Access Mode: Out of Band
		SNTP IP List (Polling Period:  Not Set): Not Set
	Drive Information
		 Enclosure - Slot 1
			Chl:  12
			SCSI ID:  0
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZTM02S6Q0000C105
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 2
			Chl:  12
			SCSI ID:  1
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1S5AE0000C103
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 3
			Chl:  12
			SCSI ID:  2
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZTN00D4N0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 4
			Chl:  12
			SCSI ID:  3
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1JFBG0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 5
			Chl:  12
			SCSI ID:  4
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZL29TATQ0000C106
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 6
			Chl:  12
			SCSI ID:  5
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1BH3R0000C017
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 7
			Chl:  12
			SCSI ID:  6
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1F92K0000C105
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 8
			Chl:  12
			SCSI ID:  7
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZTN00EV20000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 9
			Chl:  12
			SCSI ID:  8
			Size(MB):  11443968
			Status:  Media Scan 97%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1SQK40000C104
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 10
			Chl:  12
			SCSI ID:  9
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1Q0530000C102
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 11
			Chl:  12
			SCSI ID:  10
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZTN00EVX0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 12
			Chl:  12
			SCSI ID:  11
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZL29S1XS0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 13
			Chl:  12
			SCSI ID:  12
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1Q0240000C102
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 14
			Chl:  12
			SCSI ID:  13
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZL2822TZ0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 15
			Chl:  12
			SCSI ID:  14
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZTN00DHR0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 16
			Chl:  12
			SCSI ID:  15
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW16VRM0000C102
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 17
			Chl:  12
			SCSI ID:  16
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1GT3E0000C105
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 18
			Chl:  12
			SCSI ID:  17
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1CNGX0000C101
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 19
			Chl:  12
			SCSI ID:  18
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW104P30000C025
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 20
			Chl:  12
			SCSI ID:  19
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZTN00EBY0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 21
			Chl:  12
			SCSI ID:  20
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZTN00D330000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 22
			Chl:  12
			SCSI ID:  21
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1V91Z0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 23
			Chl:  12
			SCSI ID:  22
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZTN00AXQ0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 24
			Chl:  12
			SCSI ID:  23
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1S1XY0000C103
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 25
			Chl:  12
			SCSI ID:  24
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW0342W0000C104
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 26
			Chl:  12
			SCSI ID:  25
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1Q0G40000C102
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 27
			Chl:  12
			SCSI ID:  26
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW170KF0000C024
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 28
			Chl:  12
			SCSI ID:  27
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZL25J69Z0000C102
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 29
			Chl:  12
			SCSI ID:  28
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1ATJ40000C105
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 30
			Chl:  12
			SCSI ID:  29
			Size(MB):  11443968
			Status:  Media Scan 98%  pass 0
			Speed:  1200MB
			LD:  214C9D16
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1CCXD0000C102
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 31
			Chl:  12
			SCSI ID:  30
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1CMBK0000C105
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 32
			Chl:  12
			SCSI ID:  31
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZL29DH020000C105
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 33
			Chl:  12
			SCSI ID:  32
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZL29S2DD0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 34
			Chl:  12
			SCSI ID:  33
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZS8004BN0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 35
			Chl:  12
			SCSI ID:  34
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW035R80000C034
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 36
			Chl:  12
			SCSI ID:  35
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZL202HVK0000C105
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 37
			Chl:  12
			SCSI ID:  36
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZTN00ESE0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 38
			Chl:  12
			SCSI ID:  37
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1S2EP0000C103
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 39
			Chl:  12
			SCSI ID:  38
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZTN00DZD0000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 40
			Chl:  12
			SCSI ID:  39
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZL27B4VA0000C101
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 41
			Chl:  12
			SCSI ID:  40
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZL29SRG90000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 42
			Chl:  12
			SCSI ID:  41
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1SEED0000C041
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 43
			Chl:  12
			SCSI ID:  42
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1PHAD0000C105
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 44
			Chl:  12
			SCSI ID:  43
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZL29T9860000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 45
			Chl:  12
			SCSI ID:  44
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZTN00B570000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 46
			Chl:  12
			SCSI ID:  45
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1Q0MS0000C102
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 47
			Chl:  12
			SCSI ID:  46
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1EDYP0000C025
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 48
			Chl:  12
			SCSI ID:  47
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW171C60000C015
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 49
			Chl:  12
			SCSI ID:  48
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1YWSE0000C110
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 50
			Chl:  12
			SCSI ID:  49
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1BTYX0000C102
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 51
			Chl:  12
			SCSI ID:  50
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZL29TP2Z0000C015
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 52
			Chl:  12
			SCSI ID:  51
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1R11B0000C102
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 53
			Chl:  12
			SCSI ID:  52
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1EG2Q0000C105
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 54
			Chl:  12
			SCSI ID:  53
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1DYVJ0000C102
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 55
			Chl:  12
			SCSI ID:  54
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1FGRZ0000C034
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 56
			Chl:  12
			SCSI ID:  55
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW0YNE50000C105
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 57
			Chl:  12
			SCSI ID:  56
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1YYK00000C110
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 58
			Chl:  12
			SCSI ID:  57
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW17XZ10000C107
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 59
			Chl:  12
			SCSI ID:  58
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZL26K6R10000C047
			Disk Capacity (blocks): 23437770751
		 Enclosure - Slot 60
			Chl:  12
			SCSI ID:  59
			Size(MB):  11443968
			Status:  Media Scan 96%  pass 0
			Speed:  1200MB
			LD:  34770113
			Vender and Product ID: SEAGATE ST12000NM002G
			Revision Number: E003
			Serial Number: ZLW1LJHK0000C104
			Disk Capacity (blocks): 23437770751
	Logical Drive Setting(s)
		Logical Drive: Logical_Drive_1
			ID: 214C9D16
			Pool: 60Bay1A
			RAID Level: RAID 6
			Size (MB): 320431104
			Stripe Size (KB): 128
			Assignment: Slot A
			Status: Good
			Sed Security: Disabled
			Member Disk List (slot): 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 
			Volume
				Index: 0
					Name: Partition 1
					Offset(MB): 0
					Size(MB): 320431104
		Logical Drive: Logical_Drive_1
			ID: 34770113
			Pool: 60Bay1B
			RAID Level: RAID 6
			Size (MB): 320431104
			Stripe Size (KB): 128
			Assignment: Slot B
			Status: Good
			Sed Security: Disabled
			Member Disk List (slot): 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 
			Volume
				Index: 0
					Name: Partition 1
					Offset(MB): 0
					Size(MB): 320431104
	Pool Information
		Pool: 60Bay1B
			ID: 073A3C0A0835A6A7
			Size (MB): 320431104
			Assignment: Slot B
			Member: LD 34770113
			Sed Security: Disabled
			Space utilization thresholds:
				 70%: Post Notification Events
				 95%: Post Warning Events
				 96%: Post Warning Events
				 97%: Post Warning Events
				 98%: Post Warning Events
				 99%: Post Warning Events
			Volume
				Name: Volume_1
					ID: 3BCCEC891D90A8D9
					Index: 0
					Size(MB): 320374784
					Type: Block
					Status: OK
					Is Thin provisioning: no
					Map Information
						Channel: 4
							Lun: 1
							Scsi Id: 112
						Channel: 4
							Lun: 5
							Scsi Id: 112
						Channel: 4
							Lun: 1
							Scsi Id: 113
						Channel: 4
							Lun: 4
							Scsi Id: 113
						Channel: 5
							Lun: 1
							Scsi Id: 112
						Channel: 5
							Lun: 4
							Scsi Id: 112
						Channel: 5
							Lun: 1
							Scsi Id: 113
						Channel: 5
							Lun: 3
							Scsi Id: 113
						Channel: 5
							Lun: 5
							Scsi Id: 113
						Channel: 6
							Lun: 1
							Scsi Id: 112
						Channel: 6
							Lun: 4
							Scsi Id: 112
						Channel: 6
							Lun: 1
							Scsi Id: 113
						Channel: 6
							Lun: 4
							Scsi Id: 113
						Channel: 7
							Lun: 1
							Scsi Id: 112
						Channel: 7
							Lun: 4
							Scsi Id: 112
						Channel: 7
							Lun: 1
							Scsi Id: 113
						Channel: 7
							Lun: 4
							Scsi Id: 113
					Cloud Connection: No
		Pool: 60Bay1A
			ID: 753E854F7109F811
			Size (MB): 320431104
			Assignment: Slot A
			Member: LD 214C9D16
			Sed Security: Disabled
			Space utilization thresholds:
				 70%: Post Notification Events
				 95%: Post Warning Events
				 96%: Post Warning Events
				 97%: Post Warning Events
				 98%: Post Warning Events
				 99%: Post Warning Events
			Volume
				Name: Volume_1
					ID: 4C88813D4C53EFBF
					Index: 0
					Size(MB): 320381216
					Type: Block
					Status: OK
					Is Thin provisioning: no
					Map Information
						Channel: 4
							Lun: 0
							Scsi Id: 112
						Channel: 4
							Lun: 0
							Scsi Id: 113
						Channel: 5
							Lun: 0
							Scsi Id: 112
						Channel: 5
							Lun: 0
							Scsi Id: 113
						Channel: 6
							Lun: 0
							Scsi Id: 112
						Channel: 6
							Lun: 0
							Scsi Id: 113
						Channel: 7
							Lun: 0
							Scsi Id: 112
						Channel: 7
							Lun: 0
							Scsi Id: 113
					Cloud Connection: No
	Channel Setting(s)
		Channel 0
			Channel ID
				MCS Group: 0
				AID: 0
				BID: 1
			Channel Type: iSCSI
			Channel Mode: Host
			Data Service: Block-level Data Service
			Current Data Rate:
		Channel 1
			Channel ID
				MCS Group: 1
				AID: 0
				BID: 1
			Channel Type: iSCSI
			Channel Mode: Host
			Data Service: Block-level Data Service
			Current Data Rate:
		Channel 2
			Channel ID
				MCS Group: 2
				AID: 0
				BID: 1
			Channel Type: LAN
			Channel Mode: Host
			Data Service: File-level Data Service
			Current Data Rate:
		Channel 3
			Channel ID
				MCS Group: 3
				AID: 0
				BID: 1
			Channel Type: LAN
			Channel Mode: Host
			Data Service: File-level Data Service
			Current Data Rate:
		Channel 4
			Channel ID
				AID: 112
					 Port Name:210400D0230B8F23, Node Name:200000D0230B8F23
				BID: 113
					 Port Name:210400D0231B8F23, Node Name:200000D0231B8F23
			Channel Type: Fibre
			Channel Mode: Host
			Data Service:
			Current Data Rate:
			Host Board
				Slot A: FC 16G (SN: 9147244 (0x8B936C))
				Slot B: FC 16G (SN: 9147235 (0x8B9363))
			WWPN Port Name
				Slot A
				Slot B
		Channel 5
			Channel ID
				AID: 112
					 Port Name:210500D0230B8F23, Node Name:200000D0230B8F23
				BID: 113
					 Port Name:210500D0231B8F23, Node Name:200000D0231B8F23
			Channel Type: Fibre
			Channel Mode: Host
			Data Service:
			Current Data Rate:
			Host Board
				Slot A: FC 16G (SN: 9147244 (0x8B936C))
				Slot B: FC 16G (SN: 9147235 (0x8B9363))
			WWPN Port Name
				Slot A
				Slot B
		Channel 6
			Channel ID
				AID: 112
					 Port Name:210600D0230B8F23, Node Name:200000D0230B8F23
				BID: 113
					 Port Name:210600D0231B8F23, Node Name:200000D0231B8F23
			Channel Type: Fibre
			Channel Mode: Host
			Data Service:
			Current Data Rate:
			Host Board
				Slot A: FC 16G (SN: 9147244 (0x8B936C))
				Slot B: FC 16G (SN: 9147235 (0x8B9363))
			WWPN Port Name
				Slot A
				Slot B
		Channel 7
			Channel ID
				AID: 112
					 Port Name:210700D0230B8F23, Node Name:200000D0230B8F23
				BID: 113
					 Port Name:210700D0231B8F23, Node Name:200000D0231B8F23
			Channel Type: Fibre
			Channel Mode: Host
			Data Service:
			Current Data Rate: 16.0 Gbps
			Host Board
				Slot A: FC 16G (SN: 9147244 (0x8B936C))
				Slot B: FC 16G (SN: 9147235 (0x8B9363))
			WWPN Port Name
				Slot A
					 Port Name:1000001086052D78, Node Name:2000001086052D78
				Slot B
		Channel 13
			Channel Type: PCI-E
			Channel Mode: RCCOM
			Current Data Rate: 64 Gbps
	Host LUN List
		Channel 0
			SCSI ID 0
			SCSI ID 1
		Channel 1
			SCSI ID 0
			SCSI ID 1
		Channel 2
			SCSI ID 0
			SCSI ID 1
		Channel 3
			SCSI ID 0
			SCSI ID 1
	WWN Name List
	IQN List
	Host-Side Parameters
		Maximum Queued I/O Count: 1024
		LUNs per Host SCSI ID: 32 LUNs
		Login Authentication with CHAP: Disable
		Jumbo Frames: Disable
		Max Concurrent Host-LUN Connections: 4
		Tags Reserved per Host-LUN Connection: 4
		Peripheral Device Type: (TYPE = 0XD) Enclosure Services Device
		Peripheral Device Qualifier: Connected
		Device Supports Removable Media: Disable
		LUN Applicability: First Undefined Lun
		Cylinder/ Head/ Sector: Default(Variable/ Variable/ Variable)
	Drive-Side Parameters
		Disk Access Delay Time(Sec): No Delay
		SAF-TE/SES Device Check Period(Sec): 30.0
		Auto Rebuild on Drive Swap(Sec): 15.0
		Disk I/O Timeout(Sec): 30.0
		Auto-Assign Global Spare Drive: Disabled
		Drive Motor Spin Up: Disabled
		SED Authentication Key: Not Set
		Maximum Tag Count: 64
		SMART: CopyAndReplace
		Power Saving Level 1: Disabled
		Power Saving Level 2: Disabled
		SSD Remaining Life Notification: 12 %
	Disk-Array Parameters
		Rebuild Priority: Normal
		Write Verify on LD Initialization: Disabled
		Write Verify on LD Rebuild: Disabled
		Write Verify on Normal Access: Disabled
		Maximum Drive Response Timeout: Disabled
		AV Optimization Mode: Disabled
		Read-ahead Option for Media Editing: 0
		Read-ahead Option for NAS File Transfer: 256k
	Caching Parameters
		Write-Back Cache: Enabled
		Sync Period: Disabled
	Communication
		COM 1
			Baud-rate: 38400
			Terminal Emulation: Enabled
		CH: 0
			IP Assign Mode: DHCP
			SlotA MAC Address: 00:D0:23:8B:8F:23
			SlotB MAC Address: 00:D0:23:9B:8F:23
			SlotA IP Address:
			SlotA Subnet Mask:
			SlotA Default Gateway:
			SlotB IP Address:
			SlotB Subnet prefix length:
			SlotB Default Gateway:
			IPV6 Assign Mode: Disabled
			SlotA IPV6 Address:
			SlotA Subnet prefix length:
			SlotA Default Gateway:
			SlotB IPV6 Address:
			SlotB Subnet prefix length:
			SlotB Default Gateway:
		CH: 1
			IP Assign Mode: DHCP
			SlotA MAC Address: 00:D0:23:4B:8F:23
			SlotB MAC Address: 00:D0:23:5B:8F:23
			SlotA IP Address:
			SlotA Subnet Mask:
			SlotA Default Gateway:
			SlotB IP Address:
			SlotB Subnet prefix length:
			SlotB Default Gateway:
			IPV6 Assign Mode: Disabled
			SlotA IPV6 Address:
			SlotA Subnet prefix length:
			SlotA Default Gateway:
			SlotB IPV6 Address:
			SlotB Subnet prefix length:
			SlotB Default Gateway:
		CH: 2
			IP Assign Mode: DHCP
			SlotA MAC Address: 00:d0:23:c9:8f:23
			SlotB MAC Address: 00:d0:23:d9:8f:23
			SlotA IP Address:
			SlotA Subnet Mask:
			SlotA Default Gateway:
			SlotB IP Address:
			SlotB Subnet prefix length:
			SlotB Default Gateway:
			IPV6 Assign Mode: Disabled
			SlotA IPV6 Address:
			SlotA Subnet prefix length:
			SlotA Default Gateway:
			SlotB IPV6 Address:
			SlotB Subnet prefix length:
			SlotB Default Gateway:
		CH: 3
			IP Assign Mode: DHCP
			SlotA MAC Address: 00:d0:23:29:8f:23
			SlotB MAC Address: 00:d0:23:39:8f:23
			SlotA IP Address:
			SlotA Subnet Mask:
			SlotA Default Gateway:
			SlotB IP Address:
			SlotB Subnet prefix length:
			SlotB Default Gateway:
			IPV6 Assign Mode: Disabled
			SlotA IPV6 Address:
			SlotA Subnet prefix length:
			SlotA Default Gateway:
			SlotB IPV6 Address:
			SlotB Subnet prefix length:
			SlotB Default Gateway:
		LAN: 0
			IP Assign Mode: Static
			MAC Address: 00:d0:23:09:8f:23
			IP Address: 192.168.1.72
			Subnet Mask: 255.255.255.0
			Default Gateway:
			IPV6 Assign Mode: Disabled
			IPV6 Address:
			Subnet prefix length:
			Default Gateway:
		Net Protocols
			All:  Enabled
			Telnet:  Disabled
			HTTP:  Disabled
			HTTPS:  Disabled
			FTP:  Disabled
			SSH:  Disabled
			Out-of-band agent :  Enabled
			Out-of-band agent (SSL):  Enabled
			SNMP:  Enabled
			DHCP:  Enabled
			PING:  Enabled
			Discovery:  Enabled
	Trigger
		Controller Failure: Disable
		CBM Lower or Failure: Enable
		Power Supply Failed: Disable
		Fan Failure: Disable
		Temperature exceeds threshold: Disable
	Threshold
		CPU Temperature: 61.5 C
			Lower Bound: 0.0 C 
			Upper Bound: 88.0 C 
		Controller Temperature: 55.0 C
			Lower Bound: 0.0 C 
			Upper Bound: 90.0 C 
		+5V Value: 5.022 V
			Lower Bound: 4.5 V 
			Upper Bound: 5.5 V 
		+12V Value: 12.026 V
			Lower Bound: 10.8 V 
			Upper Bound: 13.2 V 
	Redundant
		Redundant Configuration: Failback complete
	Shutdown Configuration
		Shutdown Status: No pending or previously issued shutdown command
	(In Raid) Task List 
		ID:  6
			Job:  Media Scan, Logical drive 214C9D16 Priority: Low
			Period:  2 Weeks
			Start-time:  Tue May 11 01:26:29 GMT-08:00 2021
		ID:  7
			Job:  Media Scan, Logical drive 34770113 Priority: Low
			Period:  2 Weeks
			Start-time:  Tue May 11 01:29:52 GMT-08:00 2021
	Pair List
	Remote Media Extent List
	License Information List
		License Type: Thin provisioning
			Due To Expire: No due day
		License Type: Snapshot
			Image Amount (Partition/Subsystem): 64/128
			Due To Expire: No due day
		License Type: Volume Copy
			Pair Amount (Partition/Subsystem): 4/16
			Due To Expire: No due day
		License Type: Volume Mirror
			Pair Amount (Partition/Subsystem): 4/16
			Due To Expire: No due day
		License Type: Maximum Number of Expansion Enclosure per Chain
			Max JBOD Size: 15
			Due To Expire: No due day
		License Type: Self-Encryption Drives
			Due To Expire: N/A
		License Type: EonCloud Gateway
			Version: Standard
