- GS 3060R2L Array (192.168.1.72)
  - System Information
    - Controller Time: 09/05/2023 10:25 AM
    - Configuration password: Yes
    - Maintenance password: Yes
    - Total Cache Size: 128GB (ECC DDR)
    - Firmware Version: 1.49C.14
    - BIOS Version 1.11H
    - Event Version: 20201127
    - Controller Position: Slot A
    - Service ID: 9146147
    - Slot A Serial Number: 9148029
    - Slot B Serial Number: 9148028
    - Cache Backup Module: Cache Backup Module charging OFF (battery fully charged)
    - Cache Backup Module (Redundant): Cache Backup Module charging OFF (battery fully charged)
    - ID of NVRAM Defaults: V2.85.300
    - Host Board - Slot A: FC 16G (SN: 9147244 (0x8B936C))
    - Host Board - Slot B: FC 16G (SN: 9147235 (0x8B9363))
    - I2C Device
      - Device Name: PSU0
      - Value:
      - Status: PSU0 functioning normally
    - I2C Device
      - Device Name: PSU1
      - Value:
      - Status: PSU1 functioning normally
    - I2C Device
      - Device Name: Cooling Fan0
      - Value:
      - Status: Cooling Fan0 is in lowest speed
    - I2C Device
      - Device Name: Cooling Fan1
      - Value:
      - Status: Cooling Fan1 is in lowest speed
    - I2C Device
      - Device Name: Cooling Fan2
      - Value:
      - Status: Cooling Fan2 is in lowest speed
    - I2C Device
      - Device Name: Cooling Fan3
      - Value:
      - Status: Cooling Fan3 is in lowest speed
    - I2C Device
      - Device Name: Backplane Temperature
      - Value: 48.0 C
      - Status: Temp. within safe range
    - Controller Device (Redundant)
      - Device Name: CPU Temperature (Redundant)
      - Value: 59.0 C
      - Status: Temp. within safe range
    - Controller Device (Redundant)
      - Device Name: Controller Temperature(1) (Redundant)
      - Value: 53.0 C
      - Status: Temp. within safe range
    - Controller Device (Redundant)
      - Device Name: Controller Temperature(2) (Redundant)
      - Value: 62.0 C
      - Status: Temp. within safe range
    - Controller Device (Redundant)
      - Device Name: Controller Temperature(3) (Redundant)
      - Value: 62.5 C
      - Status: Temp. within safe range
    - Controller Device (Redundant)
      - Device Name: +5V Value (Redundant)
      - Value: 5.056 V
      - Status: Voltage within acceptable range
    - Controller Device (Redundant)
      - Device Name: +12V Value (Redundant)
      - Value: 12.161 V
      - Status: Voltage within acceptable range
    - Controller Device (Redundant)
      - Device Name: FC 16G (Redundant)
      - Value:
      - Status: FC 16G functioning normally
    - Controller Device
      - Device Name: CPU Temperature
      - Value: 61.0 C
      - Status: Temp. within safe range
    - Controller Device
      - Device Name: Controller Temperature(1)
      - Value: 55.0 C
      - Status: Temp. within safe range
    - Controller Device
      - Device Name: Controller Temperature(2)
      - Value: 56.0 C
      - Status: Temp. within safe range
    - Controller Device
      - Device Name: Controller Temperature(3)
      - Value: 67.0 C
      - Status: Temp. within safe range
    - Controller Device
      - Device Name: +5V Value
      - Value: 5.016 V
      - Status: Voltage within acceptable range
    - Controller Device
      - Device Name: +12V Value
      - Value: 12.013 V
      - Status: Voltage within acceptable range
    - Controller Device
      - Device Name: FC 16G
      - Value:
      - Status: FC 16G functioning normally
  - Controller Setting(s)
    - Controller Name: Not Set
    - Logo: GS 3060
    - Model: GS 3060R2L
    - Vendor: Infortrend
    - Raid Unique Identifier: 757539(0xB8F23)
    - Time Zone: -08:00
    - Date/Time: 2023-09-05 10:25
    - Access Mode: Out of Band
    - SNTP IP List (Polling Period: Not Set): Not Set
  - Drive Information
    - Enclosure - Slot 1
      - Chl: 12
      - SCSI ID: 0
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZTM02S6Q0000C105
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 2
      - Chl: 12
      - SCSI ID: 1
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1S5AE0000C103
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 3
      - Chl: 12
      - SCSI ID: 2
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZTN00D4N0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 4
      - Chl: 12
      - SCSI ID: 3
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1JFBG0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 5
      - Chl: 12
      - SCSI ID: 4
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZL29TATQ0000C106
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 6
      - Chl: 12
      - SCSI ID: 5
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1BH3R0000C017
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 7
      - Chl: 12
      - SCSI ID: 6
      - Size(MB): 11443968
      - Status: Media Scan 97% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1F92K0000C105
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 8
      - Chl: 12
      - SCSI ID: 7
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZTN00EV20000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 9
      - Chl: 12
      - SCSI ID: 8
      - Size(MB): 11443968
      - Status: Media Scan 97% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1SQK40000C104
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 10
      - Chl: 12
      - SCSI ID: 9
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1Q0530000C102
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 11
      - Chl: 12
      - SCSI ID: 10
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZTN00EVX0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 12
      - Chl: 12
      - SCSI ID: 11
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZL29S1XS0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 13
      - Chl: 12
      - SCSI ID: 12
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1Q0240000C102
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 14
      - Chl: 12
      - SCSI ID: 13
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZL2822TZ0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 15
      - Chl: 12
      - SCSI ID: 14
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZTN00DHR0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 16
      - Chl: 12
      - SCSI ID: 15
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW16VRM0000C102
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 17
      - Chl: 12
      - SCSI ID: 16
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1GT3E0000C105
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 18
      - Chl: 12
      - SCSI ID: 17
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1CNGX0000C101
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 19
      - Chl: 12
      - SCSI ID: 18
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW104P30000C025
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 20
      - Chl: 12
      - SCSI ID: 19
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZTN00EBY0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 21
      - Chl: 12
      - SCSI ID: 20
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZTN00D330000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 22
      - Chl: 12
      - SCSI ID: 21
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1V91Z0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 23
      - Chl: 12
      - SCSI ID: 22
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZTN00AXQ0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 24
      - Chl: 12
      - SCSI ID: 23
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1S1XY0000C103
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 25
      - Chl: 12
      - SCSI ID: 24
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW0342W0000C104
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 26
      - Chl: 12
      - SCSI ID: 25
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1Q0G40000C102
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 27
      - Chl: 12
      - SCSI ID: 26
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW170KF0000C024
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 28
      - Chl: 12
      - SCSI ID: 27
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZL25J69Z0000C102
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 29
      - Chl: 12
      - SCSI ID: 28
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1ATJ40000C105
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 30
      - Chl: 12
      - SCSI ID: 29
      - Size(MB): 11443968
      - Status: Media Scan 98% pass 0
      - Speed: 1200MB
      - LD: 214C9D16
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1CCXD0000C102
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 31
      - Chl: 12
      - SCSI ID: 30
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1CMBK0000C105
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 32
      - Chl: 12
      - SCSI ID: 31
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZL29DH020000C105
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 33
      - Chl: 12
      - SCSI ID: 32
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZL29S2DD0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 34
      - Chl: 12
      - SCSI ID: 33
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZS8004BN0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 35
      - Chl: 12
      - SCSI ID: 34
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW035R80000C034
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 36
      - Chl: 12
      - SCSI ID: 35
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZL202HVK0000C105
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 37
      - Chl: 12
      - SCSI ID: 36
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZTN00ESE0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 38
      - Chl: 12
      - SCSI ID: 37
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1S2EP0000C103
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 39
      - Chl: 12
      - SCSI ID: 38
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZTN00DZD0000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 40
      - Chl: 12
      - SCSI ID: 39
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZL27B4VA0000C101
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 41
      - Chl: 12
      - SCSI ID: 40
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZL29SRG90000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 42
      - Chl: 12
      - SCSI ID: 41
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1SEED0000C041
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 43
      - Chl: 12
      - SCSI ID: 42
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1PHAD0000C105
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 44
      - Chl: 12
      - SCSI ID: 43
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZL29T9860000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 45
      - Chl: 12
      - SCSI ID: 44
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZTN00B570000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 46
      - Chl: 12
      - SCSI ID: 45
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1Q0MS0000C102
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 47
      - Chl: 12
      - SCSI ID: 46
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1EDYP0000C025
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 48
      - Chl: 12
      - SCSI ID: 47
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW171C60000C015
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 49
      - Chl: 12
      - SCSI ID: 48
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1YWSE0000C110
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 50
      - Chl: 12
      - SCSI ID: 49
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1BTYX0000C102
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 51
      - Chl: 12
      - SCSI ID: 50
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZL29TP2Z0000C015
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 52
      - Chl: 12
      - SCSI ID: 51
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1R11B0000C102
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 53
      - Chl: 12
      - SCSI ID: 52
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1EG2Q0000C105
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 54
      - Chl: 12
      - SCSI ID: 53
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1DYVJ0000C102
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 55
      - Chl: 12
      - SCSI ID: 54
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1FGRZ0000C034
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 56
      - Chl: 12
      - SCSI ID: 55
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW0YNE50000C105
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 57
      - Chl: 12
      - SCSI ID: 56
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1YYK00000C110
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 58
      - Chl: 12
      - SCSI ID: 57
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW17XZ10000C107
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 59
      - Chl: 12
      - SCSI ID: 58
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZL26K6R10000C047
      - Disk Capacity (blocks): 23437770751
    - Enclosure - Slot 60
      - Chl: 12
      - SCSI ID: 59
      - Size(MB): 11443968
      - Status: Media Scan 96% pass 0
      - Speed: 1200MB
      - LD: 34770113
      - Vender and Product ID: SEAGATE ST12000NM002G
      - Revision Number: E003
      - Serial Number: ZLW1LJHK0000C104
      - Disk Capacity (blocks): 23437770751
  - Logical Drive Setting(s)
    - Logical Drive: Logical_Drive_1
      - ID: 214C9D16
      - Pool: 60Bay1A
      - RAID Level: RAID 6
      - Size (MB): 320431104
      - Stripe Size (KB): 128
      - Assignment: Slot A
      - Status: Good
      - Sed Security: Disabled
      - Member Disk List (slot): 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30,
      - Volume
        - Index: 0
          - Name: Partition 1
          - Offset(MB): 0
          - Size(MB): 320431104
    - Logical Drive: Logical_Drive_1
      - ID: 34770113
      - Pool: 60Bay1B
      - RAID Level: RAID 6
      - Size (MB): 320431104
      - Stripe Size (KB): 128
      - Assignment: Slot B
      - Status: Good
      - Sed Security: Disabled
      - Member Disk List (slot): 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60,
      - Volume
        - Index: 0
          - Name: Partition 1
          - Offset(MB): 0
          - Size(MB): 320431104
  - Pool Information
    - Pool: 60Bay1B
      - ID: 073A3C0A0835A6A7
      - Size (MB): 320431104
      - Assignment: Slot B
      - Member: LD 34770113
      - Sed Security: Disabled
      - Space utilization thresholds:
        - 70%: Post Notification Events
        - 95%: Post Warning Events
        - 96%: Post Warning Events
        - 97%: Post Warning Events
        - 98%: Post Warning Events
        - 99%: Post Warning Events
      - Volume
        - Name: Volume_1
          - ID: 3BCCEC891D90A8D9
          - Index: 0
          - Size(MB): 320374784
          - Type: Block
          - Status: OK
          - Is Thin provisioning: no
          - Map Information
            - Channel: 4
              - Lun: 1
              - Scsi Id: 112
            - Channel: 4
              - Lun: 5
              - Scsi Id: 112
            - Channel: 4
              - Lun: 1
              - Scsi Id: 113
            - Channel: 4
              - Lun: 4
              - Scsi Id: 113
            - Channel: 5
              - Lun: 1
              - Scsi Id: 112
            - Channel: 5
              - Lun: 4
              - Scsi Id: 112
            - Channel: 5
              - Lun: 1
              - Scsi Id: 113
            - Channel: 5
              - Lun: 3
              - Scsi Id: 113
            - Channel: 5
              - Lun: 5
              - Scsi Id: 113
            - Channel: 6
              - Lun: 1
              - Scsi Id: 112
            - Channel: 6
              - Lun: 4
              - Scsi Id: 112
            - Channel: 6
              - Lun: 1
              - Scsi Id: 113
            - Channel: 6
              - Lun: 4
              - Scsi Id: 113
            - Channel: 7
              - Lun: 1
              - Scsi Id: 112
            - Channel: 7
              - Lun: 4
              - Scsi Id: 112
            - Channel: 7
              - Lun: 1
              - Scsi Id: 113
            - Channel: 7
              - Lun: 4
              - Scsi Id: 113
          - Cloud Connection: No
    - Pool: 60Bay1A
      - ID: 753E854F7109F811
      - Size (MB): 320431104
      - Assignment: Slot A
      - Member: LD 214C9D16
      - Sed Security: Disabled
      - Space utilization thresholds:
        - 70%: Post Notification Events
        - 95%: Post Warning Events
        - 96%: Post Warning Events
        - 97%: Post Warning Events
        - 98%: Post Warning Events
        - 99%: Post Warning Events
      - Volume
        - Name: Volume_1
          - ID: 4C88813D4C53EFBF
          - Index: 0
          - Size(MB): 320381216
          - Type: Block
          - Status: OK
          - Is Thin provisioning: no
          - Map Information
            - Channel: 4
              - Lun: 0
              - Scsi Id: 112
            - Channel: 4
              - Lun: 0
              - Scsi Id: 113
            - Channel: 5
              - Lun: 0
              - Scsi Id: 112
            - Channel: 5
              - Lun: 0
              - Scsi Id: 113
            - Channel: 6
              - Lun: 0
              - Scsi Id: 112
            - Channel: 6
              - Lun: 0
              - Scsi Id: 113
            - Channel: 7
              - Lun: 0
              - Scsi Id: 112
            - Channel: 7
              - Lun: 0
              - Scsi Id: 113
          - Cloud Connection: No
  - Channel Setting(s)
    - Channel 0
      - Channel ID
        - MCS Group: 0
        - AID: 0
        - BID: 1
      - Channel Type: iSCSI
      - Channel Mode: Host
      - Data Service: Block-level Data Service
      - Current Data Rate:
    - Channel 1
      - Channel ID
        - MCS Group: 1
        - AID: 0
        - BID: 1
      - Channel Type: iSCSI
      - Channel Mode: Host
      - Data Service: Block-level Data Service
      - Current Data Rate:
    - Channel 2
      - Channel ID
        - MCS Group: 2
        - AID: 0
        - BID: 1
      - Channel Type: LAN
      - Channel Mode: Host
      - Data Service: File-level Data Service
      - Current Data Rate:
    - Channel 3
      - Channel ID
        - MCS Group: 3
        - AID: 0
        - BID: 1
      - Channel Type: LAN
      - Channel Mode: Host
      - Data Service: File-level Data Service
      - Current Data Rate:
    - Channel 4
      - Channel ID
        - AID: 112
          - Port Name:210400D0230B8F23, Node Name:200000D0230B8F23
        - BID: 113
          - Port Name:210400D0231B8F23, Node Name:200000D0231B8F23
      - Channel Type: Fibre
      - Channel Mode: Host
      - Data Service:
      - Current Data Rate:
      - Host Board
        - Slot A: FC 16G (SN: 9147244 (0x8B936C))
        - Slot B: FC 16G (SN: 9147235 (0x8B9363))
      - WWPN Port Name
        - Slot A
        - Slot B
    - Channel 5
      - Channel ID
        - AID: 112
          - Port Name:210500D0230B8F23, Node Name:200000D0230B8F23
        - BID: 113
          - Port Name:210500D0231B8F23, Node Name:200000D0231B8F23
      - Channel Type: Fibre
      - Channel Mode: Host
      - Data Service:
      - Current Data Rate:
      - Host Board
        - Slot A: FC 16G (SN: 9147244 (0x8B936C))
        - Slot B: FC 16G (SN: 9147235 (0x8B9363))
      - WWPN Port Name
        - Slot A
        - Slot B
    - Channel 6
      - Channel ID
        - AID: 112
          - Port Name:210600D0230B8F23, Node Name:200000D0230B8F23
        - BID: 113
          - Port Name:210600D0231B8F23, Node Name:200000D0231B8F23
      - Channel Type: Fibre
      - Channel Mode: Host
      - Data Service:
      - Current Data Rate:
      - Host Board
        - Slot A: FC 16G (SN: 9147244 (0x8B936C))
        - Slot B: FC 16G (SN: 9147235 (0x8B9363))
      - WWPN Port Name
        - Slot A
        - Slot B
    - Channel 7
      - Channel ID
        - AID: 112
          - Port Name:210700D0230B8F23, Node Name:200000D0230B8F23
        - BID: 113
          - Port Name:210700D0231B8F23, Node Name:200000D0231B8F23
      - Channel Type: Fibre
      - Channel Mode: Host
      - Data Service:
      - Current Data Rate: 16.0 Gbps
      - Host Board
        - Slot A: FC 16G (SN: 9147244 (0x8B936C))
        - Slot B: FC 16G (SN: 9147235 (0x8B9363))
      - WWPN Port Name
        - Slot A
          - Port Name:1000001086052D78, Node Name:2000001086052D78
        - Slot B
    - Channel 13
      - Channel Type: PCI-E
      - Channel Mode: RCCOM
      - Current Data Rate: 64 Gbps
  - Host LUN List
    - Channel 0
      - SCSI ID 0
      - SCSI ID 1
    - Channel 1
      - SCSI ID 0
      - SCSI ID 1
    - Channel 2
      - SCSI ID 0
      - SCSI ID 1
    - Channel 3
      - SCSI ID 0
      - SCSI ID 1
  - WWN Name List
  - IQN List
  - Host-Side Parameters
    - Maximum Queued I/O Count: 1024
    - LUNs per Host SCSI ID: 32 LUNs
    - Login Authentication with CHAP: Disable
    - Jumbo Frames: Disable
    - Max Concurrent Host-LUN Connections: 4
    - Tags Reserved per Host-LUN Connection: 4
    - Peripheral Device Type: (TYPE = 0XD) Enclosure Services Device
    - Peripheral Device Qualifier: Connected
    - Device Supports Removable Media: Disable
    - LUN Applicability: First Undefined Lun
    - Cylinder/ Head/ Sector: Default(Variable/ Variable/ Variable)
  - Drive-Side Parameters
    - Disk Access Delay Time(Sec): No Delay
    - SAF-TE/SES Device Check Period(Sec): 30.0
    - Auto Rebuild on Drive Swap(Sec): 15.0
    - Disk I/O Timeout(Sec): 30.0
    - Auto-Assign Global Spare Drive: Disabled
    - Drive Motor Spin Up: Disabled
    - SED Authentication Key: Not Set
    - Maximum Tag Count: 64
    - SMART: CopyAndReplace
    - Power Saving Level 1: Disabled
    - Power Saving Level 2: Disabled
    - SSD Remaining Life Notification: 12 %
  - Disk-Array Parameters
    - Rebuild Priority: Normal
    - Write Verify on LD Initialization: Disabled
    - Write Verify on LD Rebuild: Disabled
    - Write Verify on Normal Access: Disabled
    - Maximum Drive Response Timeout: Disabled
    - AV Optimization Mode: Disabled
    - Read-ahead Option for Media Editing: 0
    - Read-ahead Option for NAS File Transfer: 256k
  - Caching Parameters
    - Write-Back Cache: Enabled
    - Sync Period: Disabled
  - Communication
    - COM 1
      - Baud-rate: 38400
      - Terminal Emulation: Enabled
    - CH: 0
      - IP Assign Mode: DHCP
      - SlotA MAC Address: 00:D0:23:8B:8F:23
      - SlotB MAC Address: 00:D0:23:9B:8F:23
      - SlotA IP Address:
      - SlotA Subnet Mask:
      - SlotA Default Gateway:
      - SlotB IP Address:
      - SlotB Subnet prefix length:
      - SlotB Default Gateway:
      - IPV6 Assign Mode: Disabled
      - SlotA IPV6 Address:
      - SlotA Subnet prefix length:
      - SlotA Default Gateway:
      - SlotB IPV6 Address:
      - SlotB Subnet prefix length:
      - SlotB Default Gateway:
    - CH: 1
      - IP Assign Mode: DHCP
      - SlotA MAC Address: 00:D0:23:4B:8F:23
      - SlotB MAC Address: 00:D0:23:5B:8F:23
      - SlotA IP Address:
      - SlotA Subnet Mask:
      - SlotA Default Gateway:
      - SlotB IP Address:
      - SlotB Subnet prefix length:
      - SlotB Default Gateway:
      - IPV6 Assign Mode: Disabled
      - SlotA IPV6 Address:
      - SlotA Subnet prefix length:
      - SlotA Default Gateway:
      - SlotB IPV6 Address:
      - SlotB Subnet prefix length:
      - SlotB Default Gateway:
    - CH: 2
      - IP Assign Mode: DHCP
      - SlotA MAC Address: 00:d0:23:c9:8f:23
      - SlotB MAC Address: 00:d0:23:d9:8f:23
      - SlotA IP Address:
      - SlotA Subnet Mask:
      - SlotA Default Gateway:
      - SlotB IP Address:
      - SlotB Subnet prefix length:
      - SlotB Default Gateway:
      - IPV6 Assign Mode: Disabled
      - SlotA IPV6 Address:
      - SlotA Subnet prefix length:
      - SlotA Default Gateway:
      - SlotB IPV6 Address:
      - SlotB Subnet prefix length:
      - SlotB Default Gateway:
    - CH: 3
      - IP Assign Mode: DHCP
      - SlotA MAC Address: 00:d0:23:29:8f:23
      - SlotB MAC Address: 00:d0:23:39:8f:23
      - SlotA IP Address:
      - SlotA Subnet Mask:
      - SlotA Default Gateway:
      - SlotB IP Address:
      - SlotB Subnet prefix length:
      - SlotB Default Gateway:
      - IPV6 Assign Mode: Disabled
      - SlotA IPV6 Address:
      - SlotA Subnet prefix length:
      - SlotA Default Gateway:
      - SlotB IPV6 Address:
      - SlotB Subnet prefix length:
      - SlotB Default Gateway:
    - LAN: 0
      - IP Assign Mode: Static
      - MAC Address: 00:d0:23:09:8f:23
      - IP Address: 192.168.1.72
      - Subnet Mask: 255.255.255.0
      - Default Gateway:
      - IPV6 Assign Mode: Disabled
      - IPV6 Address:
      - Subnet prefix length:
      - Default Gateway:
    - Net Protocols
      - All: Enabled
      - Telnet: Disabled
      - HTTP: Disabled
      - HTTPS: Disabled
      - FTP: Disabled
      - SSH: Disabled
      - Out-of-band agent : Enabled
      - Out-of-band agent (SSL): Enabled
      - SNMP: Enabled
      - DHCP: Enabled
      - PING: Enabled
      - Discovery: Enabled
  - Trigger
    - Controller Failure: Disable
    - CBM Lower or Failure: Enable
    - Power Supply Failed: Disable
    - Fan Failure: Disable
    - Temperature exceeds threshold: Disable
  - Threshold
    - CPU Temperature: 62.5 C
      - Lower Bound: 0.0 C
      - Upper Bound: 88.0 C
    - Controller Temperature: 55.0 C
      - Lower Bound: 0.0 C
      - Upper Bound: 90.0 C
    - +5V Value: 5.022 V
      - Lower Bound: 4.5 V
      - Upper Bound: 5.5 V
    - +12V Value: 12.026 V
      - Lower Bound: 10.8 V
      - Upper Bound: 13.2 V
  - Redundant
    - Redundant Configuration: Failback complete
  - Shutdown Configuration
    - Shutdown Status: No pending or previously issued shutdown command
  - (In Raid) Task List
    - ID: 6
      - Job: Media Scan, Logical drive 214C9D16 Priority: Low
      - Period: 2 Weeks
      - Start-time: Tue May 11 01:26:29 GMT-08:00 2021
    - ID: 7
      - Job: Media Scan, Logical drive 34770113 Priority: Low
      - Period: 2 Weeks
      - Start-time: Tue May 11 01:29:52 GMT-08:00 2021
  - Pair List
  - Remote Media Extent List
  - License Information List
    - License Type: Thin provisioning
      - Due To Expire: No due day
    - License Type: Snapshot
      - Image Amount (Partition/Subsystem): 64/128
      - Due To Expire: No due day
    - License Type: Volume Copy
      - Pair Amount (Partition/Subsystem): 4/16
      - Due To Expire: No due day
    - License Type: Volume Mirror
      - Pair Amount (Partition/Subsystem): 4/16
      - Due To Expire: No due day
    - License Type: Maximum Number of Expansion Enclosure per Chain
      - Max JBOD Size: 15
      - Due To Expire: No due day
    - License Type: Self-Encryption Drives
      - Due To Expire: N/A
    - License Type: EonCloud Gateway
      - Version: Standard